SR760 ANALYZE MENU.VI
  Front Panel
    - trace 0 analyze.# sidebands uses data range coercion, which now only applies to data entry; values will not be coerced when passed to subVIs.  To coerce passed values,  use the In Range and Coerce function.
    - active trace # uses data range coercion, which now only applies to data entry; values will not be coerced when passed to subVIs.  To coerce passed values,  use the In Range and Coerce function.
    - trace 1 analyze.# sidebands uses data range coercion, which now only applies to data entry; values will not be coerced when passed to subVIs.  To coerce passed values,  use the In Range and Coerce function.
SR760 AVERAGE MENU.VI
  Front Panel
    - average.overlap uses data range coercion, which now only applies to data entry; values will not be coerced when passed to subVIs.  To coerce passed values,  use the In Range and Coerce function.
    - average.# averages uses data range coercion, which now only applies to data entry; values will not be coerced when passed to subVIs.  To coerce passed values,  use the In Range and Coerce function.
SR760 DATA TABLE.VI
  Front Panel
    - active trace # uses data range coercion, which now only applies to data entry; values will not be coerced when passed to subVIs.  To coerce passed values,  use the In Range and Coerce function.
SR760 DATA TRANSFER.VI
  Front Panel
    - active trace uses data range coercion, which now only applies to data entry; values will not be coerced when passed to subVIs.  To coerce passed values,  use the In Range and Coerce function.
SR760 DISPLAY MENU.VI
  Front Panel
    - active trace # uses data range coercion, which now only applies to data entry; values will not be coerced when passed to subVIs.  To coerce passed values,  use the In Range and Coerce function.
SR760 FREQUENCY MENU.VI
  Front Panel
    - starting band uses data range coercion, which now only applies to data entry; values will not be coerced when passed to subVIs.  To coerce passed values,  use the In Range and Coerce function.
SR760 GLOBAL.VI
  Front Panel
    - input range uses data range coercion, which now only applies to data entry; values will not be coerced when passed to subVIs.  To coerce passed values,  use the In Range and Coerce function.
    - Y/Div uses data range coercion, which now only applies to data entry; values will not be coerced when passed to subVIs.  To coerce passed values,  use the In Range and Coerce function.
    - table index uses data range coercion, which now only applies to data entry; values will not be coerced when passed to subVIs.  To coerce passed values,  use the In Range and Coerce function.
SR760 INPUT MENU.VI
  Front Panel
    - trigger & auto functions.delay uses data range coercion, which now only applies to data entry; values will not be coerced when passed to subVIs.  To coerce passed values,  use the In Range and Coerce function.
    - trigger & auto functions.trigger level uses data range coercion, which now only applies to data entry; values will not be coerced when passed to subVIs.  To coerce passed values,  use the In Range and Coerce function.
    - input.input range uses data range coercion, which now only applies to data entry; values will not be coerced when passed to subVIs.  To coerce passed values,  use the In Range and Coerce function.
SR760 LIMIT TABLE.VI
  Front Panel
    - active trace uses data range coercion, which now only applies to data entry; values will not be coerced when passed to subVIs.  To coerce passed values,  use the In Range and Coerce function.
SR760 MEASURE MENU.VI
  Front Panel
    - trace 0 measure.EU scaling uses data range coercion, which now only applies to data entry; values will not be coerced when passed to subVIs.  To coerce passed values,  use the In Range and Coerce function.
    - active trace # uses data range coercion, which now only applies to data entry; values will not be coerced when passed to subVIs.  To coerce passed values,  use the In Range and Coerce function.
    - trace 1 measure.EU scaling uses data range coercion, which now only applies to data entry; values will not be coerced when passed to subVIs.  To coerce passed values,  use the In Range and Coerce function.
SR760 SCALE MENU.VI
  Front Panel
    - trace 1 scale.Y/Div uses data range coercion, which now only applies to data entry; values will not be coerced when passed to subVIs.  To coerce passed values,  use the In Range and Coerce function.
    - trace 1 scale.left bin uses data range coercion, which now only applies to data entry; values will not be coerced when passed to subVIs.  To coerce passed values,  use the In Range and Coerce function.
    - trace 0 scale.Y/Div uses data range coercion, which now only applies to data entry; values will not be coerced when passed to subVIs.  To coerce passed values,  use the In Range and Coerce function.
    - trace 0 scale.left bin uses data range coercion, which now only applies to data entry; values will not be coerced when passed to subVIs.  To coerce passed values,  use the In Range and Coerce function.
    - active trace # uses data range coercion, which now only applies to data entry; values will not be coerced when passed to subVIs.  To coerce passed values,  use the In Range and Coerce function.
SR770EG.VI
  Front Panel
    - trigger & auto functions.delay uses data range coercion, which now only applies to data entry; values will not be coerced when passed to subVIs.  To coerce passed values,  use the In Range and Coerce function.
    - trigger & auto functions.trigger level uses data range coercion, which now only applies to data entry; values will not be coerced when passed to subVIs.  To coerce passed values,  use the In Range and Coerce function.
    - trace 0 scale.trace 0 scale.Y/Div uses data range coercion, which now only applies to data entry; values will not be coerced when passed to subVIs.  To coerce passed values,  use the In Range and Coerce function.
    - trace 0 scale.trace 0 scale.left bin uses data range coercion, which now only applies to data entry; values will not be coerced when passed to subVIs.  To coerce passed values,  use the In Range and Coerce function.
    - trace 0 analyze.# sidebands uses data range coercion, which now only applies to data entry; values will not be coerced when passed to subVIs.  To coerce passed values,  use the In Range and Coerce function.
    - trace 1 analyze.# sidebands uses data range coercion, which now only applies to data entry; values will not be coerced when passed to subVIs.  To coerce passed values,  use the In Range and Coerce function.
    - trace 1 measure.EU scaling uses data range coercion, which now only applies to data entry; values will not be coerced when passed to subVIs.  To coerce passed values,  use the In Range and Coerce function.
    - average.overlap uses data range coercion, which now only applies to data entry; values will not be coerced when passed to subVIs.  To coerce passed values,  use the In Range and Coerce function.
    - average.# averages uses data range coercion, which now only applies to data entry; values will not be coerced when passed to subVIs.  To coerce passed values,  use the In Range and Coerce function.
    - active trace # uses data range coercion, which now only applies to data entry; values will not be coerced when passed to subVIs.  To coerce passed values,  use the In Range and Coerce function.
    - input.input range uses data range coercion, which now only applies to data entry; values will not be coerced when passed to subVIs.  To coerce passed values,  use the In Range and Coerce function.
    -  marker.move marker to bin # uses data range coercion, which now only applies to data entry; values will not be coerced when passed to subVIs.  To coerce passed values,  use the In Range and Coerce function.
    - trace 0 measure.EU scaling uses data range coercion, which now only applies to data entry; values will not be coerced when passed to subVIs.  To coerce passed values,  use the In Range and Coerce function.
    - frequency.starting band uses data range coercion, which now only applies to data entry; values will not be coerced when passed to subVIs.  To coerce passed values,  use the In Range and Coerce function.
    - trace 1 scale.trace 1 scale.Y/Div uses data range coercion, which now only applies to data entry; values will not be coerced when passed to subVIs.  To coerce passed values,  use the In Range and Coerce function.
    - trace 1 scale.trace 1 scale.left bin uses data range coercion, which now only applies to data entry; values will not be coerced when passed to subVIs.  To coerce passed values,  use the In Range and Coerce function.
