SR760 GLOBAL.VI
  Front Panel
    - input range uses data range coercion, which now only applies to data entry; values will not be coerced when passed to subVIs.  To coerce passed values,  use the In Range and Coerce function.
    - Y/Div uses data range coercion, which now only applies to data entry; values will not be coerced when passed to subVIs.  To coerce passed values,  use the In Range and Coerce function.
    - table index uses data range coercion, which now only applies to data entry; values will not be coerced when passed to subVIs.  To coerce passed values,  use the In Range and Coerce function.
