{"text_format":"2","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":6,"n_cols":19,"rows_kept":6,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
[null,"R(Ohm)or T(mK)",null,"T(mK)/or R(Ohm)"]
[null,null,null,"Do not enter data below",null,null,"X",null,"A","B1","B2","B3","B4","B5","B6","B7","B8","B9","Y"]
[]
["10K (r-T) (R in kOhm)",30.623,null,1662.7917223131453,null,null,1.4860477343578256,null,6909.169478051,-38314.105969326,93795.121719782,-132881.190697614,120024.664196962,-71674.983797385,28300.34446649,-7125.704599868,1038.446472548,-66.75479913,3.2208378538407487]
["Dale 1562",9300,null,39.187028309614824,null,null,3.9684829485539352,null,204421460.76087,-491699863.206724,525071687.631145,-326724128.255054,130552659.264214,-34739757.2702707,6156089.97375606,-700530.051818518,46451.046674688,-1367.454854768,1.593142330646515]
["Pt1000-RT-12-380K",50,null,38.451800743373944,null,null,1.6989700043360187,null,-469.544790033,2142.429105073,-4278.355519358,4917.129912473,-3583.140137551,1717.059717072,-541.269035711,108.277676198,-12.478784052,0.631579503,1.584916683138701]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}